ANNEX  E
AVAILABLE TRANSMISSION CAPACITY

	
Connection Point/Voltage Level
	Available Transmission Capacity for GEA-6,
Cumulative MW (as of January 2026)

	
	2027
	2028
	2029
	2030

	LUZON
	3,034
	3,134
	4,334
	5,234

	I. Existing
	2,224
	2,224
	2,224
	2,224

	Tap to Bauang-San Fabian 69 kV Line
	40
	40
	40
	40

	Bacnotan 69 kV SS
	60
	60
	60
	60

	Tap to La Trinidad-Sagada 69 kV Line
	60
	60
	60
	60

	Tap to San Manuel-Calasiao 69 kV Line
	80
	80
	80
	80

	Tap to Nagsaag-Umingan 69 kV Line
	40
	40
	40
	40

	Tap to Labrador-San Carlos 69 kV Line
	40
	40
	40
	40

	Tap to Labrador-Bani 69 kV Line
	40
	40
	40
	40

	Balingueo 230 kV S/S
	60
	60
	60
	60

	Balsik 230 kV S/S
	300
	300
	300
	300

	Mariveles (Alas-asin) 500 kV S/S
	584
	584
	584
	584

	Tap to Mexico-Calumpit 69 kV Line
	40
	40
	40
	40

	Tap to Mexico-Apalit 69 kV Line
	90
	90
	90
	90

	Tap to Cabanatuan-San Luis 69 kV Line
	40
	40
	40
	40

	San Jose 230 kV S/S
	400
	400
	400
	400

	Tap to Batangas-Rosario 69 kV Line
	40
	40
	40
	40

	Tap to Batangas-Mabini-Cuenca 69 kV Line
	40
	40
	40
	40

	Tap to Bay-Calamba 69 kV Line
	40
	40
	40
	40

	Tap to Gumaca-Pitogo-Mulanay 69 kV Line
	40
	40
	40
	40

	Labo 69 kV S/S
	0
	0
	0
	0

	Tap to Tiwi C-Malinao 69 kV Line
	30
	30
	30
	30

	Tap to Daraga-Irosin 69 kV Line
	40
	40
	40
	40

	Tap to Daraga-Ligao 69 kV Line
	40
	40
	40
	40

	Tap to Naga-Iriga 69 kV Line
	40
	40
	40
	40

	Tap to Daraga-Sto. Domingo 69 kV Line
	40
	40
	40
	40

	II. Proposed
	810
	910
	2,110
	3,010

	Balaoan 500 kV SS
	0
	0
	0
	0

	Laoag 500/230 kV SS
	0
	0
	0
	0

	Castillejos 230 kV S/S
	190
	460
	460
	460

	Porac 230 kV S/S
	0
	0
	300
	300

	Tuy 230 kV S/S
	620
	450
	450
	450

	Milaor 500 kV S/S
	0
	0
	900
	1,800

	Sta. Maria 50 kV S/S
	0
	0
	0
	0



Page 1 of 4

	
Connection Point/Voltage Level
	Available Transmission Capacity for GEA-6,
Cumulative MW (as of January 2026)

	
	2027
	2028
	2029
	2030

	VISAYAS
	810
	810
	2,192
	2,442

	I. Existing
	120
	120
	1,502
	1,752

	Dumanjug 230 kV S/S
	0
	0
	300
	300

	Dumanjug 69 kV S/S
	0
	0
	90
	90

	Toledo 138 kV S/S
	0
	0
	40
	40

	Naga 138 kV S/S
	0
	0
	150
	150

	Tap to Calong-calong- Asturias 69 kV T/L
	40
	40
	40
	40

	Corella 230 kV S/S
	0
	0
	600
	600

	Corella 138kV S/S
	0
	0
	150
	150

	Corella 69 kV S/S
	0
	0
	52
	52

	Ubay 138 kV S/S
	0
	0
	0
	250

	Tap to Corella-Tagbilaran 69 kV T/L
	40
	40
	40
	40

	Tap to Corella-Maribojoc 69 kV T/L
	40
	40
	40
	40

	II. Proposed
	690
	690
	690
	690

	Tominjao 230 kV SWS
	0
	0
	0
	0

	Umapad 230 kV S/S
	600
	600
	600
	600

	Umapad 69 kV S/S
	90
	90
	90
	90

	Bonbon 230 kV SWS
	0
	0
	0
	0



	
Connection Point/Voltage Level
	Available Transmission Capacity for GEA-6,
Cumulative MW (as of January 2026)

	
	2027
	2028
	2029
	2030

	MINDANAO
	3,240
	3,240
	3,240
	3,290

	I. Existing
	2,640
	2,640
	2,640
	2,690

	Polanco–Roxas 69 kV Transmission Line
	40
	40
	40
	40

	Tap to Aurora-Calamba 69 kV Line
	40
	40
	40
	40

	Tap to Aurora-San Miguel 69 kV Line
	40
	40
	40
	40

	Tap to Zamboanga-Tumaga 69 kV Line
	40
	40
	40
	40

	Aurora 69 kV SS
	20
	20
	20
	20

	Pitogo 69 kV SS
	40
	40
	40
	40

	Zamboanga 69 kV SS
	20
	20
	20
	20

	Tap to Agus 6-Kauswagan 69 kV Line
	20
	20
	20
	20

	Lala 230 kV SS
	300
	300
	300
	300

	Balo-i 230 kV SS
	150
	150
	150
	150

	Balo-I 69 kV SS
	40
	40
	40
	40

	Tap to Jasaan-Balingasag 69 kV Line
	40
	40
	40
	40

	Maramag 230 kV SS
	300
	300
	300
	300

	Villanueva 230 kV SS
	150
	150
	150
	150

	Opol 138 kV SS
	50
	50
	50
	100

	Jasaan 138 kV SS
	100
	100
	100
	100

	Kibawe 138 kV SS
	100
	100
	100
	100

	Manolo Fortich 69 kV SS
	40
	40
	40
	40

	Opol 69 kV SS
	40
	40
	40
	40

	Tagoloan 69 kV SS
	40
	40
	40
	40

	Maramag 69 kV SS
	40
	40
	40
	40

	Placer 138 kV SS
	70
	70
	70
	70

	San Francisco 138 kV SS
	150
	150
	150
	150

	San Francisco 69 kV SS
	40
	40
	40
	40

	Tap to Nabunturan-Asuncion 69 kV Line
	40
	40
	40
	40

	Tap to Nabunturan-Compostela 69 kV Line
	40
	40
	40
	40

	Tap to Maco-Banaybanay 69 kV Line
	40
	40
	40
	40

	Tap to Maco-Tagum 69 kV Line
	40
	40
	40
	40

	Toril 230 kV SS
	300
	300
	300
	300

	Maramag 69 kV SS
	40
	40
	40
	40

	Davao 69 kV SS
	40
	40
	40
	40

	Bunawan 69 kV SS
	40
	40
	40
	40

	Tap to Sultan Kudarat-Datu Saudi Ampatuan 69 kV Line
	40
	40
	40
	40

	Tap to Tacurong-Salbu 69 kV Line
	40
	40
	40
	40

	Tacurong 138kV SS
	20
	20
	20
	20



	
Connection Point/Voltage Level
	Available Transmission Capacity for GEA-6, Cumulative MW (as of January 2026)

	
	2027
	2028
	2029
	2030

	Tap to Tacurong-Kalamansig 69 kkV SS Line
	50
	50
	50
	50

	II. Proposed
	600
	600
	600
	600

	Laguindingan 230 kV SS
	300
	300
	300
	300

	Kabacan 138 kV SS
	150
	150
	150
	150

	Koronadal 138 kV SS
	0
	0
	0
	0

	Tago 138 kV SS
	150
	150
	150
	150

	Mati 69 kV SS
	0
	0
	0
	0

	Mati 138 kV SS
	0
	0
	0
	0



